ORC – questionnaire

For a preliminary assessment of the possible generation of electricity when organizing the organic Rankine cycle , please provide the following data:

	№ p /p
	Parameter
	Unit of measurement
	Value to fill

	1. 
	Heat source (heat carrier)

(exhaust gases, geothermal water, etc.)
	-
	

	2. 
	Heat carrier flowrate
	st.m3 /h
( kg / h)
	

	3. 
	Temperature of the heat carrier at the inlet
	° C
	

	4. 
	Heat carrier outlet temperature (if applicable)
	° C
	

	5. 
	Heat carrier pressure at the inlet
	bar g
	

	6. 
	Heat carrier outlet pressure (if applicable)
	bar g
	

	7. 
	Required electrical network parameters for connection

(240V / 50Hz, 400V/50Hz, 6300V/50Hz etc.)
	V/ Hz
	

	8. 
	Preferred medium for the organic Rankine cycle ( thermal oil , cyclopentane , etc.)
	-
	

	9. 
	Equipment placement

(open area, indoor)
	-
	

	10. 
	Equipment placement location (climate)
	-
	

	11. 
	Availability of utilities on the equipment placement site and their parameters (instrument air, water for heat exchangers) (pressure, inlet / outlet temperature , flow rate)
	bar g ,

°C/ °C,

m3 /h
	


